- Qt Creator Documentation
- Add a QNX Neutrino device
- Qt Creator 19.0.0-beta2

Developing for QNX Neutrino devices ◦ Create kits for QNX Neutrino devices

# Add a QNX Neutrino device

You can use a wizard to add a QNX Neutrino device, or add one manually.

## Use a wizard to add a device

To use a wizard to add QNX Device:

1. Go to Preferences > Devices > Devices.
2. Select Add > QNX Device > Start Wizard.

3. In The name to identify this configuration, enter a name for the connection.
4. In The device's host name or IP address, enter the host name or IP address of the device. This becomes the value of the `%{Device:HostAddress}` variable.
5. In The device's SSH port number, enter the port number for SSH connections. This becomes the value of the `%{Device:SshPort}` variable.
6. In The username to log into the device, enter the username to log into the device and run the application. This becomes the value of the `%{Device:UserName}` variable.
7. Select Next to open the Key Deployment dialog.

8. In Private key file, select a private key file for authentication. This becomes the value of the `%{Device:PrivateKeyFile}` variable.
9. If you don't have a public-private key pair, select Create New Key Pair. For more information, see Generate SSH keys.
10. Select Deploy Public Key to copy the public key to the device.
11. Select Next to create the connection.

To change device preferences, go to Preferences > Devices > Devices and select a device in Device.

## Manually add a device

To add a device without using the wizard, select QNX Device in the pull-down menu of the Add button.

See also Developing for QNX Neutrino devices, How to: Develop for QNX, How to: Develop for remote Linux, and How to: Manage kits.

Developing for QNX Neutrino devices ◦ Create kits for QNX Neutrino devices